|  |
| --- |
| **Magnetic LED Strips Quotation****2016 V10.0** |
|   |
| **No.** | **ITEM** | **DESCRIPTION** | **WATTS** | **The price included** | **Lumens& Effeciency** | **DIMENSION** |  |  |  |
|  |  |  |  |  |
| **1** | **WL-RTST124** | **1.AC100-277V**1. **LED:SMD 2835**

**Bridgelux**1. **Driver: UL Class II 4.CCT:4000K/5000K**

**5.Lens:Clear/Frost** | **24W 1 ×Strip** | **1.PCB Board with LED 2.Aluminum profile 3.2× DC Wire****4.2× Nuts**1. **Lens (Clear or Frost)**
2. **L Shape bracket 7.2×Magnet per strip**
 | **125-135Lm/W****2500-2700Lm** | **4 Feet (****L44.5''×W0.71''H0.54'')** |  |  |  |  |  |
| **2** | **WL-RTST230** | **30W 2×Strips** | **125-135Lm/W****3750-4050Lm** |  |  |  |  |  |
| **3** | **WL-RTST240** | **40W 2×Strips** | **125-135Lm/W****5000-5400Lm** |  |  |  |  |  |
| **4** | **WL-RTST345** | **45W 3×Strips** | **125-135Lm/W****5625-6075Lm** |  |  |  |  |  |
| **5** | **WL-RTST360** | **60W 3×Strips** | **125-135Lm/W****7500-8100Lm** |  |  |  |  |  |
| **6** | **WL-RTST460** | **60W 4×Strips** | **125-135Lm/W****7500-8100Lm** |  |  |  |  |  |
| **7** | **WL-RTST480** | **80W 4×Strips** | **125-135Lm/W****10000-10800Lm** |  |  |  |  |  |
| **8** | **WL-RTST2120** | **20W 1 ×Strip** | **125-135Lm/W****2500-2700Lm** | **2 Feet (L22.2''×W0.71''H0.54'')** |  |  |  |  |  |
| **9** | **WL-RTST2230** | **30W 2×Strips** | **125-135Lm/W****3750-4050Lm** |  |  |  |  |  |
| **10** | **WL-RTST2340** | **40W 3×Strips** | **125-135Lm/W****5000-5400Lm** |  |  |  |  |  |
| **1.Price Term:EX-Work 2.Quotation valid:60 days 3.Warranty 5 years****4.Non-flicker driver is avaialbe.** |

